**GPU Computing Project Report**

David Sevic

January 2025

**Design Methodology**

Chosen algorithm

The chosen algorithm for this project is the Barnes-Hut approximation of N-body simulations.

N-body simulation involves a number of steps, during which, bodies (particles) are moving in a given dimension space, by interacting with all other bodies through gravitational forces. Each body has its own: mass, position and velocity. Body mass is constant throughout the simulation, while velocities and positions are changed after each simulation step.

These are the formulas used for N-body simulation:

<formula for force>


<formula for calculating acceleration>

<formula for updating velocity>

<formula for updating positions>

The algorithm can be viewed as two parts: calculation of forces and updating of the bodies (velocities and positions). The naïve approach for calculating forces involves summing up all of the forces from other bodies to the current one, and this approach has the complexity of N^2.

Barnes-Hut approximation is an optimization of the naïve approach, where instead of calculating forces between all other bodies, some groups of distant bodies are treated as a single body, and therefore the complexity is reduced to N\*logN. The version of the Barnes-Hut approximation in this project uses a quadtree structure in order to represent the bodies. A quadtree is a type of tree that divides a 2D space into quadrants. Nodes are either parent nodes with 4 children nodes, or leaf nodes representing region without further division.



<https://opendsa-server.cs.vt.edu/ODSA/Books/CS3/html/_images/PRexamp.png>

In the Barnes-Hut approximation, quadtree is used to store bodies into quadrants based on their position in the 2D space. When calculating the forces, quadtree is traversed for each body and based on a given threshold parameter, only quadrants which are close enough are divided all the way to the leaf nodes, and those quadrants that are distant enough, are treated as a single body, and therefore the complexity is reduced.

The creation of quadtree can be performed in parallel, however for this project, this part is left sequential, which does affect the overall results (more about this in the results section).

The force calculations are applied to each body independently and this is where parallelism can be efficiently utilized. After calculating the forces, the updating of the bodies’ velocities and positions is also done independently for each body and is therefore also perfectly parallelizable.

The code used for quadtree creation and traversing is created by taking motivation from available pseudo code (https://patterns.eecs.berkeley.edu/?page\_id=193#Barnes\_Hut).

Creating quadtree

The quadtree in this project is represented as an array in memory, consisted of quadrants.

**const** **int** QUADRANT\_SIZE = **12**;

**const** **int** CHILDREN\_0 = **0**;

**const** **int** CHILDREN\_1 = **1**;

**const** **int** CHILDREN\_2 = **2**;

**const** **int** CHILDREN\_3 = **3**;

**const** **int** CENTER\_OF\_MASS\_X = **4**;

**const** **int** CENTER\_OF\_MASS\_Y = **5**;

**const** **int** TOTAL\_MASS = **6**;

**const** **int** X\_MIN = **7**;

**const** **int** X\_MAX = **8**;

**const** **int** Y\_MIN = **9**;

**const** **int** Y\_MAX = **10**;

**const** **int** PARTICLE\_INDEX = **11**;

**const** **double** THETA = **5e-1**;

**const** **int** QUADTREE\_MAX\_DEPTH = **10**;

**const** **int** QUADTREE\_MAX\_SIZE = **static\_cast**<**int**>(pow(**4**, QUADTREE\_MAX\_DEPTH));

**using** Quadrant = std::array<**double**, QUADRANT\_SIZE>;

std::vector<Quadrant> quadtree;


Each quadrant is consisted of 12 different fields:


* 4 fields for children
* X and Y coordinates of quadrant center of mass
* Total mass of the quadrant
* Min and Max coordinates of the quadrant
* Index of the particle(body) in the quadrant

For increased precision, we are using type double. However, float could be used, and therefore half the size of the quadtree in memory.

Initially, for the CPU implementation, the quadtree did not have the maximum depth limit. However, when we started with the GPU implementation and usage of shared memory, we had to limit the maximum size of the quadtree, in order to fit into the available hardware memory. Because of this limit, it is possible and quite often the case, that multiple particles will end up in the same leaf node at maximum depth, which does not divide further. Implementation wise, this requested some changes in the initial logic, and algorithm wise this does not present an issue, because this type of aggregation is already happening in case of distant quadrants.

The other predefined limit QUADTREE\_MAX\_SIZE presents a practical maximum number of quadrants in the quadtree and is set to 4^QUADTREE\_MAX\_DEPTH. The reason for this is that in the worst case scenario, when all of the bodies are distant enough, at each level of the tree, there will be particles in all 4 children nodes. In our project, this is the case in the initial and possibly few early stages, because initially, the positions of the bodies are random and evenly distributed over the space. In the later simulation steps, due to some bodies being heavier, the lighter bodies will move towards them, and eventually the tree becomes sparse, having less quadrants. For the given values of max depth of 10, max number of 4^10 quadrants and each quadrant having 12 double values; the maximum memory of the quadtree is around 96MB, which is not even close to the available shared memory. Therefore, depending on number of bodies, the quadtree might not fit into shared memory in one or few early simulation steps, until it becomes sparse enough.





The first image shows the quadtree in the initial state, where all the bodies are evenly spread out across the quadrants. The second image shows quadtree in the last simulation step, where most of the bodies have been drawn to the heaviest ones, and therefore the quadtree has much less quadrants. The red dots represent quadrants with at least one body inside. We say at least, because after adding the max depth limit, some quadrants end up having multiple bodies inside of them, and since we don’t need information about which particles are inside of these max depth quadrants, in order to save memory, we can only present them as one red dot.

The quadtree is initially created with a root quadrant, covering the whole 2D space which is used to initialize positions of the bodies. After that, each body is inserted in a sequence. The insertion of bodies is complex, and it consists of finding the quadrant in which the inserting body belongs, and then if this quadrant is already occupied, dividing it into 4 children nodes (if less than max allowed depth), and reassigning the previous leaf node body as one of the children. Because of this dynamic approach, if bodies were to be inserted in parallel, it would cause conflicts between in the situations when the leaf nodes are divided, and bodies are reassigned. However, there are other approaches which are parallel friendly, such as encoding bodies with Morton Code, then sorting them out and creating subtrees at different levels in parallel. This is one of the ways in which this project could be improved.

std::vector<Quadrant> buildTree(**const** Positions& positions, **const** Masses& masses) {

quadtree.clear();

std::array<**double**, **4**> rootBounds = ComputeRootBounds(positions);

**double** xMin = rootBounds[**0**];

**double** xMax = rootBounds[**1**];

**double** yMin = rootBounds[**2**];

**double** yMax = rootBounds[**3**];

InitializeRoot(xMin, xMax, yMin, yMax);

**for** (**int** i = **0**; i < N\_BODIES; ++i) {

QuadInsert(i, **0**, positions, masses, **1**);

}

ComputeMass(**0**);

**return** quadtree;

}

After creating the quadtree, one additional traverse is performed, in order to compute the center and total mass of each quadrant. There is a different approach, where this can be done on the fly, while traversing the body in the force computing part, and therefore increasing time complexity, but saving memory space for storing this information. In this project, we stuck to the motivational CPU implementation, where it was done in this way.