**GPU Computing Project Report**

David Sevic

January 2025

**Design Methodology**

Chosen algorithm

The chosen algorithm for this project is the Barnes-Hut approximation of N-body simulations.

N-body simulation involves a number of steps, during which, bodies (particles) are moving in a given dimension space, by interacting with all other bodies through gravitational forces. Each body has its own: mass, position and velocity. Body mass is constant throughout the simulation, while velocities and positions are changed after each simulation step.

These are the formulas used for N-body simulation:

<formula for force>


<formula for calculating acceleration>

<formula for updating velocity>

<formula for updating positions>

The algorithm can be viewed as two parts: calculation of forces and updating of the bodies (velocities and positions). The naïve approach for calculating forces involves summing up all of the forces from other bodies to the current one, and this approach has the complexity of N^2.

Barnes-Hut approximation is an optimization of the naïve approach, where instead of calculating forces between all other bodies, some groups of distant bodies are treated as a single body, and therefore the complexity is reduced to N\*logN. The version of the Barnes-Hut approximation in this project uses a quadtree structure in order to represent the bodies. A quadtree is a type of tree that divides a 2D space into quadrants. Nodes are either parent nodes with 4 children nodes, or leaf nodes representing region without further division.



<https://opendsa-server.cs.vt.edu/ODSA/Books/CS3/html/_images/PRexamp.png>

In the Barnes-Hut approximation, quadtree is used to store bodies into quadrants based on their position in the 2D space. When calculating the forces, quadtree is traversed for each body and based on a given threshold parameter, only quadrants which are close enough are divided all the way to the leaf nodes, and those quadrants that are distant enough, are treated as a single body, and therefore the complexity is reduced.

The creation of quadtree can be performed in parallel, however for this project, this part is left sequential, which does affect the overall results (more about this in the results section).

The force calculations are applied to each body independently and this is where parallelism can be efficiently utilized. After calculating the forces, the updating of the bodies’ velocities and positions is also done independently for each body and is therefore also perfectly parallelizable.

The code used for quadtree creation and traversing is created by taking motivation from available pseudo code (https://patterns.eecs.berkeley.edu/?page\_id=193#Barnes\_Hut).

Creating quadtree

The quadtree in this project is represented as an array in memory, consisted of quadrants.

**const** **int** QUADRANT\_SIZE = **12**;

**const** **int** CHILDREN\_0 = **0**;

**const** **int** CHILDREN\_1 = **1**;

**const** **int** CHILDREN\_2 = **2**;

**const** **int** CHILDREN\_3 = **3**;

**const** **int** CENTER\_OF\_MASS\_X = **4**;

**const** **int** CENTER\_OF\_MASS\_Y = **5**;

**const** **int** TOTAL\_MASS = **6**;

**const** **int** X\_MIN = **7**;

**const** **int** X\_MAX = **8**;

**const** **int** Y\_MIN = **9**;

**const** **int** Y\_MAX = **10**;

**const** **int** PARTICLE\_INDEX = **11**;

**const** **double** THETA = **5e-1**;

**const** **int** QUADTREE\_MAX\_DEPTH = **10**;

**const** **int** QUADTREE\_MAX\_SIZE = **static\_cast**<**int**>(pow(**4**, QUADTREE\_MAX\_DEPTH));

**using** Quadrant = std::array<**double**, QUADRANT\_SIZE>;

std::vector<Quadrant> quadtree;


Each quadrant is consisted of 12 different fields:


* 4 fields for children quadrants
* X and Y coordinates of quadrant’s center of mass
* Total mass of the quadrant
* Min and Max coordinates of the quadrant
* Index of the particle(body) in the quadrant

For increased precision, we are using type double. However, float could be used, and therefore half the size of the quadtree in memory.

Initially, for the CPU implementation, the quadtree did not have the maximum depth limit. However, when we started with the GPU implementation and usage of shared memory, we had to limit the maximum size of the quadtree in order to fit into the available hardware memory. Because of this limit, it is possible and quite often the case, that multiple particles will end up in the same leaf node at maximum depth, which does not divide further. Implementation wise, this requested some changes in the initial logic, and algorithm wise this does not present an issue, because this type of aggregation is already happening in case of distant quadrants.

The other predefined limit QUADTREE\_MAX\_SIZE presents a practical maximum number of quadrants in the quadtree and is set to (4^QUADTREE\_MAX\_DEPTH−1)/3. The reason for this is that in the worst-case scenario, when all of the bodies are distant enough, at each level of the tree, there will be particles in all 4 child nodes. This calculation accounts for the total number of quadrants in a balanced quadtree by summing the number of nodes at each level of depth. The division by 3 comes from the formula for the sum of a geometric series, ∑i=0d​4i=(4d+1−1)/3, which accurately represents the total number of quadrants in the tree across all levels. In our project, this is the case in the initial and possibly few early stages, because initially, the positions of the bodies are random and evenly distributed over the space. In the later simulation steps, due to some bodies being heavier, the lighter bodies will move towards them, and eventually, the tree becomes sparse, having fewer quadrants. For the given values of max depth of 10, the maximum number of quadrants is (4^11−1)/3, and with each quadrant having 12 double values, the maximum memory of the quadtree is around 128MB, which is not even close to the available shared memory. Therefore, depending on number of bodies, the quadtree might not fit into shared memory in one or few early simulation steps, until it becomes sparse enough.





The first image shows the quadtree in the initial state, where all the bodies are evenly spread out across the quadrants. The second image shows quadtree in the last simulation step, where most of the bodies have been drawn to the heaviest ones, and therefore the quadtree has much less quadrants. The red dots represent quadrants with at least one body inside. We say at least, because after adding the max depth limit, some quadrants end up having multiple bodies inside of them, and since we don’t need information about which particles are inside of these max depth quadrants, in order to save memory, we can only present them as one red dot.

The quadtree is initially created with a root quadrant, covering the whole 2D space which is used to initialize positions of the bodies. After that, each body is inserted in a sequence. The insertion of bodies is complex, and it consists of finding the quadrant in which the inserting body belongs, and then if this quadrant is already occupied, dividing it into 4 children nodes (if less than max allowed depth), and reassigning the previous leaf node body as one of the children. Because of this dynamic approach, if bodies were to be inserted in parallel, it would cause conflicts between in the situations when the leaf nodes are divided, and bodies are reassigned. However, there are other approaches which are parallel friendly, such as encoding bodies with Morton Code, then sorting them out and creating subtrees at different levels in parallel. This is one of the ways in which this project could be improved.

std::vector<Quadrant> buildTree(**const** Positions& positions, **const** Masses& masses) {

quadtree.clear();

std::array<**double**, **4**> rootBounds = ComputeRootBounds(positions);

**double** xMin = rootBounds[**0**];

**double** xMax = rootBounds[**1**];

**double** yMin = rootBounds[**2**];

**double** yMax = rootBounds[**3**];

InitializeRoot(xMin, xMax, yMin, yMax);

**for** (**int** i = **0**; i < N\_BODIES; ++i) {

QuadInsert(i, **0**, positions, masses, **1**);

}

ComputeMass(**0**);pip install wrapt

**return** quadtree;

}

After creating the quadtree, one additional traverse is performed, in order to compute the center and total mass of each quadrant. There is a different approach, where this can be done on the fly, while traversing the body in the force computing part, and therefore increasing time complexity, but saving memory space for storing this information. In this project, we stuck to the motivational CPU implementation, where it was done in this way.

Simulation run

The N-body simulation consists of a number of simulation steps which are perfomed in a loop. In each iteration step, we are doing the following:

loop:

create\_quadtree

allocate\_quadtree\_mem\_on\_gpu

copy\_quadtree\_from\_cpu\_to\_gpu

compute\_forces\_gpu

compute\_acc\_vel\_pos\_gpu

copy\_positions\_from\_gpu\_to\_cpu

deallocate\_quadtree\_mem\_on\_gpu

This pseudo code explains the logic of the simulation step loop, which will later be showed and explained in code. Before defining the loop in the code, it is necessary to define and allocate memory.

*// declaration of GPU memory*

**double\*** masses\_d**;**

**double\*** positions\_d**;**

**double\*** velocities\_d**;**

**double\*** accelerations\_d**;**

**double\*** forces\_d**;**

**double\*** quadtree\_d**;**

*// allocating GPU memory*

cudaMalloc**(** **(void\*\*)&**masses\_d**,** N\_BODIES **\*** **sizeof(double));**

cudaMalloc**(** **(void\*\*)&**positions\_d**,** N\_BODIES **\*** N\_DIM **\*** **sizeof(double));**

cudaMalloc**(** **(void\*\*)&**velocities\_d**,** N\_BODIES **\*** N\_DIM **\*** **sizeof(double));**

cudaMalloc**(** **(void\*\*)&**accelerations\_d**,** N\_BODIES **\*** N\_DIM **\*** **sizeof(double));**

cudaMalloc**(** **(void\*\*)&**forces\_d**,** N\_BODIES **\*** N\_DIM **\*** **sizeof(double));**

In this implementation, we are working with arrays of type double for body masses, positions, velocities and forces. Out of these, only masses contain one value per body, while the other ones contain N\_DIM values (which is always 2 in our case, since we are using a quadtree optimization; if octatree is used, then N\_DIM is equal to 3). Based on this, we are allocating the required amount of memory on GPU.

Since the quadtree is potentially changing its size in each iteration, we have to decide how to allocate its memory on GPU. One approach is to allocate memory at the start of each iteration, after building the tree on CPU, based on its exact size and then to deallocate this memory at the end of the interation. This approach allocates exact amount of required memory and therefore doesn’t take unnacessary global memory from the GPU which could be used for different purposes. However, this approach introduces both allocation and deallocation in each step of the simulation, which creates the overhead.

The other approach uses only one allocation before entering the loop of simulation steps and one deallocation after the loop. This way, avoiding the overhead of multiple allocations and deallocations. The downside is that since we have only one allocation, we need to allocate the maximum expected amount of memory for the quadtree size, and will not change it later. In this implementation, the bodies are initialized with random masses, and as steps of simulation advance, lighter bodies are drawn to heavier ones, and therefore the the quadtree becomes sparse and its size gets smaller. So the quadtree will likely achieve its maximum size right at the start and with each iteration will get smaller and smaller. However, with the second approach, we will still have maximum size allocated on GPU and part of it will be unused.

Both approaches have their upsides and downsides. After executing the program with both approaches and different parameters, we measured a nearly identical run times. With a larger number of simulation steps, the overhead of the first approach is accumulating more, however it makes a tiny bit of the total time, which is similar to the second approach. Therefore, we decided to use the second approach and avoid multiple allocations and deallocations of GPU memory, as it is generally not a good practise.

*// allocation of maximum size quadtree*

**size\_t** realistic\_size **=** std**::**min**(4** **\*** N\_BODIES**,** QUADTREE\_MAX\_SIZE**);**

cudaMalloc**(** **(void\*\*)&**quadtree\_d**,** realistic\_size **\*** **sizeof(**Quadrant**));**

At the beginning of the simulation, the positions of bodies are random and uniformly spread over the space. Because of that, the tree will be balanced with tendency of the bodies to end up as leaves of the quadtree. Therefore, we are calculating the upper limit by multiplying the number of bodies with the branching factor of 4. Becasue of the nature of this algorithm, after the first iteration, the ligher bodies are moving towards the heavier ones, making the tree sparse and therefore having a smaller size. Also, because we have the limit of maximum depth, here we need to make sure not to allocate more than allowed maximum size of the quadtree (therefore the min function).

At the beginning, each body is initialized with its mass, starting position and starting velocity. Accelerations and forces are not initialized as they are calculated later. Therefore, we have to copy the initialzied values from CPU to GPU’s allocated memory.

*// copying initial values to GPU*

cudaMemcpy**(** masses\_d**,** masses**.**data**(),** N\_BODIES **\*** **sizeof(double),** cudaMemcpyHostToDevice**);**

cudaMemcpy**(** positions\_d**,** positions**.**data**(),** N\_BODIES **\*** N\_DIM **\*** **sizeof(double),** cudaMemcpyHostToDevice**);**

cudaMemcpy**(** velocities\_d**,** velocities**.**data**(),** N\_BODIES **\*** N\_DIM **\*** **sizeof(double),** cudaMemcpyHostToDevice**);**

After this setup, we are ready to define the simulation loop. As our formulas are taking into account time steps, we are keeping track of the absolute time passed, and are increasing it at each iteration by the defined time step.

**const double** DELTA\_T **= 1.0;**

**...**

**for** **(int** step **=** **0;** step **<** N\_SIMULATIONS**;** **++**step**)** **{**

**absolute\_t** **+=** DELTA\_T**;**

**...**

At the beginning of each iteration, the first thing which is being done is creation of quadtree. As already mentioned, this computation is left out on CPU and therefore, after creating it, it has to be copied to the GPU.

*// copy tree to gpu*

cudaMemcpy**(** quadtree\_d**,** quadtree**.**data**(),** quadtree**.**size**()** **\*** **sizeof(**Quadrant**),** cudaMemcpyHostToDevice**);**

As the quadtree is shared amongst all threads, and frequently accessed, we can benefit from storing it into shared memory. Since its size is changing in each iteration, we need to calculate whether it can fit into shared memory or not.

*// calculate the quadtree size*

**int** quadtreeMemSize **=** quadtree**.**size**()** **\*** **sizeof(**Quadrant**);**

*// use shared memory if tree can fit in it*

**int** sharedMemSize **=** quadtreeMemSize **<=** MAX\_SHARED\_MEM\_PER\_BLOCK\_B **?** quadtreeMemSize **:** **0;**

We are comparing its size with the maximum available shared memory, which is 48KB for our hardware. This calculated memory will later be passed to the kernel.

For the block dimension, we decided to use 1D, since all our data is composed of 1D arrays. The block size can vary depending on whether shared memory is used or not. Since there are two limits to shared memory: per SM and per block, we can consider which block sizes to choose. In case of using global memory, each SM will be assigned with multiple blocks based on avaliable resources. Therefore, smaller blocksizes cause each SM to be assigned with more blocks, which increases its occupacy and is beneficiery. On the other hand, when using shared memory, number of blocks per SM is more restricted by the size of allocated shared memory. Since per block limit is 48KB and per SM limit is 64KB, if we allocate for example 40KB, only one block will be stored per SM. Therefore, when using shared memory, we want to use larger blocksizes, to make the most out of the SM.

*// defining blocksizes for global and shared memory cases*

**int** blockSize **=** **0;**

**if** **(**sharedMemSize **==** **0)** **{**

blockSize **=** **32;**

**}** **else** **{**

blockSize **=** **64;**

**}**

Initially, this implementation used the same number of threads as number of bodies in the simulation. However, to measure performance in more details, we changed it so that the number of threads is parametrized. Therefore, the number of blocks is calcualted concidering block size and number of threads.

*// defining dimensions*

dim3 dimBlock**(**blockSize**);**

*// depends on N\_THREADS for arbitrary number of threads approach*

dim3 dimGrid**((**N\_THREADS **+** blockSize **-** **1)** **/** blockSize**);**

Execution of the kernel code for force computation is defined by passing the calculated number and dimension of blocks, and size of shared memory. Amongst other parameters, we are passing a boolean conditional parameter sharedMemSize **>** **0**, which indicates whether or not to work with shared memory. After the kernel execution, we are synchonizing the CPU code, because we need to have the computed forces in order to proceed with the algorithm.

*// pass quadtree memory size for dynamic allocation of shared memory*

computeForcesGpu**<<<**dimGrid**,** dimBlock**,** sharedMemSize**>>>(**positions\_d**,**

masses\_d**,** forces\_d**,** quadtree\_d**,** quadtree**.**size**(),** sharedMemSize **>** **0);**

cudaDeviceSynchronize**();**

The kernel code for computation of forces starts with the declaration of sahred memory as well as calculation of the global thread id.

\_\_global\_\_ **void** computeForcesGpu**(double\*** positions**,** **double\*** masses**,** **double\*** forces**,** **double\*** globalMemQuadtree**,** **int** quadtreeNumElem**,** **bool** useSharedMem**)** **{**

*// declaration of shared memory for quadtree*

**extern** \_\_shared\_\_ **double** sharedMemQuadtree**[];**

**int** idx **=** blockIdx**.**x **\*** blockDim**.**x **+** threadIdx**.**x**;**

**if** **(**idx **>=** N\_BODIES**)**

**return;**

In order to proceed with the calculation of forces, we first need to store the quadtree from global to shared memory. This can be done in parallel, by assigning different quadtrants based on thread ids.

**if (**useSharedMem**) {**

**for** **(int** i **=** threadIdx**.**x**;** i **<** quadtreeNumElem**;** i **+=** blockDim**.**x**)** **{**

sharedMemQuadtree**[**i **\*** QUADRANT\_SIZE **+** CHILDREN\_0**]** **=** globalMemQuadtree**[**i **\*** QUADRANT\_SIZE **+** CHILDREN\_0**];**

sharedMemQuadtree**[**i **\*** QUADRANT\_SIZE **+** CHILDREN\_1**]** **=** globalMemQuadtree**[**i **\*** QUADRANT\_SIZE **+** CHILDREN\_1**];**

**...**

**}**

syncthreads**();**

**}**

All threads of a block are entering this piece of code and are responsible of transfering one quadrant each, from global to shared memory, in each iteration. For e.g. if we have a blocksize of 64 and 128 quadrants in the tree, then in the first iteration the 0th thread is transfering the 0th quadrant, 1st thread the 1st quadrant and 63rd thead the 63rd quadrant. Then in the second iteration, 0th tread is transfering the 64th quadrant, the 1st thread the 65th quadrant and 63rd thread the 127th quadrant.

After introducing usage of shared memory with this approach, the performances have not improved at all. After analysing, we realized that there is a large number of bank conflicts happening in the this approach.

If we look at the thread level, in order to transfer one quadrant from global to shared memory, it is copying all 12 fields of a quadrant. These fields are stored sequentially in memory, which means that the 0th thread is accessing banks 0-11 for transfering one quadrant. The 1st thread is accessing banks 12-23, and the 3rd thread thread is accessing banks 24-31 and 0-3, and so on. With 32 threads in a warp executing simultaneously, there is a lot of bank conflicts happening, which is affecting the performance and canceling out the advantages of shared memory.

To resolve this, we can store quadrant fields differently in shared memory. Since these are indepentant fields, and we are accessing them by index, it wouldn’t be a problem if they are not placed sequentially in memory. What we want is for each thread to access only one bank in shared memory. There are 32 banks and if we look at the 0th thread, we want it to store all 12 quadrant fields into the 0th bank, the 1st thread into 1st bank and 31st thread into 31st bank. To achieve this, we have to store the fields with offset equal to the number of banks (32 in our case), and therefore, each thread in a warp will be accessing unique bank and there will be no conflicts.

**if (**useSharedMem**) {**

**for** **(int** i **=** threadIdx**.**x**;** i **<** quadtreeNumElem**;** i **+=** blockDim**.**x**)** **{**

sharedMemQuadtree**[**i **\*** SHARED\_MEM\_BANKS\_NUM **+** CHILDREN\_0**]** **=** globalMemQuadtree**[**i **\*** QUADRANT\_SIZE **+** CHILDREN\_0**];**

sharedMemQuadtree**[**i **\*** SHARED\_MEM\_BANKS\_NUM **+** CHILDREN\_1**]** **=** globalMemQuadtree**[**i **\*** QUADRANT\_SIZE **+** CHILDREN\_1**];**

**...**

**}**

syncthreads**();**

**}**

It is true that if we are using a blocksize larger than 32, then we would have multiple threads accessing the same banks, but it is imporant to remember that seperate warps are usually not being executed simoultaniously, and therefore not causing conflicts.

This way, we have removed the write bank conflict, becase we are able to manually determine which locations will be accessed by threads based on their index. Later in the kernel code, threads are going to read from this shared memory and in an unpredictable way. Since each thread will be accessing different quadtree nodes, based on the location of the body it is processing, there will most likely be read bank conflicts, and there isn’t much we can do about it.

We have optimized the access to the shared memory in this transfer or data, however what about the global memory? When accessing global memory, there is no such thing as banks, but another important thing which is coalesced access. We want threads to access consecutive memory locations relative to each other so that the GPU can combine those transactions and minimize the latency. In the current code, each thread is accessing quadrant\_size consecutive memory locations, so the 0th thread is accessing locations 0 to 11, the 1st thread locations 12 to 23 and so on. To make this access coalesced, we want the 0th thread to access location 0, the 1st location 1 and so on.

**for** **(int** i **=** threadIdx**.**x**;** i **<** quadtreeNumElem **\*** QUADRANT\_SIZE**;** i **+=** blockDim**.**x**)** **{**

**double** val **=** globalMemQuadtree**[**i**];**

**int** quadrantIdx **=** i **/** QUADRANT\_SIZE**;**

**int** fieldIdx **=** i **%** QUADRANT\_SIZE**;**

sharedMemQuadtree**[**quadrantIdx **+** SHARED\_MEM\_BANKS\_NUM **\*** fieldIdx**]** **=** val**;**

**}**

To achieve this, we modify the loop so that we access one field at a time from the global memory. For this one field, we calculate which quadrant and field it belongs to, and then insert it into the right location in the shared memory. This way, each thread is accessing global memory locations one by one, making the access coalesced. The local variables are shown here for readability, but were removed in the actual code.

As already mentioned, in the Barnes-Hut optimization, the calculation of forces is done by traversing the quadtree. This is done for each body independently, and therefore is highly parallelizable, as it can be performed simultaneously. The straightforward approach is having threads be responsible for force calculation over one or more bodies, depending on the problem size and number of threads.

Our initial implementation used the same number of threads as bodies, where each thread processed exactly one body. We decided to change this and make number of threads a parameter as well to have an additional analysis of performance.

The tree traversal is performed as a DFS (Depth First Seach) algorigthm for which we are using a stack structure. At the begginging, the root node is pushed to the stack and a loop is entered. In the loop, we are popping a node from the stack and checking whether it should be divided futher or not. In case the node is a leaf or it is distant enough based on the approximation parameter, it is not divided further and we are calculating the force between it and the current body we are processing. In case the popped node is close enough, we are dividing it further by pushing all 4 of its children nodes to the stack. This process is repeated until the stack is empty and the traversal is finished.

*// repeat for multiple bodies*

**for(int** body\_i **=** idx**;** body\_i **<** N\_BODIES**;** body\_i **+=** N\_THREADS**)** **{**

**double** sum**[2]** **=** **{0,** **0};**

**double** pos\_i**[2]** **=** **{**positions**[**body\_i **\*** **2** **+** **0],** positions**[**body\_i **\*** **2** **+** **1]};**

**int** nodeStack**[**QUADTREE\_MAX\_DEPTH **\*** **3** **+** **1];**

**int** stack\_top **=** **-1;**

*// push the root node (rootIndex is 0)*

**if** **(!**push**(**nodeStack**,** **&**stack\_top**,** **0))** **{**

printf**(**"Stack overflow while pushing root node.\n"**);**

**return;**

**}**

**...**

The stack is implemented as an interger array, as we are storing node indexes in it. Other than storing in shared memory, another reason for limitting the maximum depth of the quadtree, was to make it possible to have an upper limit in size for the stack in kernel code. Since this stack is a local variable, it can be stored in the register memory of the thread, which has the fastest access. However, if the stack is too large, it might be placed into the global memory, which is much slower, and therefore lowering the performance. (pomeni ovo u rezultatima posle, tacne brojeve itd). There was a thought about storing this stack in a different type of memory, such as shared memory for example, however, as every thread is having a different traversal path, this wouldn’t make sense. For the stack size limit, we used QUADTREE\_MAX\_DEPTH **\*** **3** **+** **1**, because during traversal, at each level, one node is popped and maximum of 4 nodes is pushed to the stack, giving a net gain of 3 per level. On top of that, we add **+** **1**, for the root node. For stack pushing and popping, we defined seperate functions, using the \_\_device\_\_ notation to indicate these functions are used by the kernel code.

\_\_device\_\_ **bool** push**(int** stack**[],** **int** **\***top**,** **int** value**)** **{**

**if** **(\***top **>=** QUADTREE\_MAX\_DEPTH **\*** **3)** **{**

*// stack overflow*

**return** false**;**

**}**

stack**[++(\***top**)]** **=** value**;**

**return** true**;**

**}**

\_\_device\_\_ **bool** pop**(int** stack**[],** **int** **\***top**,** **int** **\***value**)** **{**

**if** **(\***top **<** **0)** **{**

*// stack underflow*

**return** false**;**

**}**

**\***value **=** stack**[(\***top**)--];**

**return** true**;**

**}**

The outer loop of each thread, is making sure the bodies are spread over the trheads in a right way, so that threads are processing multiple bodies, in case there is less of them. We are also making sure to access the quadtree with the correct indexing, based on whether shared memory was used or not.

**for(int body\_i = idx; body\_i < N\_BODIES; body\_i += N\_THREADS) {**

**...**

**while** **(**stack\_top **>=** **0)** **{**

**int** nodeIndex**;**

**if** **(!**pop**(**nodeStack**,** **&**stack\_top**,** **&**nodeIndex**))** **{**

printf**(**"Stack underflow while popping node.\n"**);**

**break;**

**}**

**double\*** node **=** useSharedMem

**?** **&**quadtree**[**nodeIndex**]**

**:** **&**quadtree**[**nodeIndex **\*** QUADRANT\_SIZE**];**

**const** **int** ACCESS\_INDEX **=** useSharedMem **?** SHARED\_MEM\_BANKS\_NUM **:** **1;**

**...**

The rest of the force computation logic is following the approach we already explained, but we did focus on one more way to optimize the kernel code. As we mentioned, the local variables in the kernel code are first attemped to be stored in the thread registers. The total number of registers is limited per SM, and by reducing the number of registers used, we are allowing more threads to be executed on an SM simultaneously and therefore increase its occupacy and overall performance.

Because of that, it is useful to observe the local variable definitions in our kernel code and see if they are necessary.

**double** pos\_i**[2]** **=** **{**positions**[**body\_i **\*** **2** **+** **0],** positions**[**body\_i **\*** **2** **+** **1]};**

**...**

displacement**[0]** **=** node**[**ACCESS\_INDEX **\*** CENTER\_OF\_MASS\_X**]** **-** pos\_i**[0];**

displacement**[1]** **=** node**[**ACCESS\_INDEX **\*** CENTER\_OF\_MASS\_Y**]** **-** pos\_i**[1];**

**...**

Some of the variables, such as pos\_i array, were initially used simply for code readability and were referenced only once after their definition. These local variables should definitelly be removed, as they introduce no computational benefits, and only take up the limited registers.

**double** sum**[2]** **=** **{0,** **0};**

**...**

**while** **(**stack\_top **>=** **0)** **{**

**...**

sum**[0]** **+=** force\_mag **\*** nx**;**

sum**[1]** **+=** force\_mag **\*** ny**;**

**...**

**}**

forces**[**body\_i **\*** **2** **+** **0]** **=** sum**[0];**

forces**[**body\_i **\*** **2** **+** **1]** **=** sum**[1];**

On the other hand, a local varaible such as sum array should not be removed. It is true that it can be replaced with direct accesses to the forces array, freeing up the registers.

forces**[**body\_i **\*** **2** **+** **0]** **=** **0;**

forces**[**body\_i **\*** **2** **+** **1]** **=** **0;**

**...**

**while** **(**stack\_top **>=** **0)** **{**

**...**

forces**[**body\_i **\*** **2** **+** **0]** **+=** force\_mag **\*** nx**;**

forces**[**body\_i **\*** **2** **+** **1]** **+=** force\_mag **\*** ny**;**

**...**

**}**

However, the forces array is stored in global memory. For each force calculation pair, this array would be accessed with 2 reads and 2 writes. Even though we are using a Barnes-Hut optimization and there are less pairings, still this is large number of global memory accesses. On the other hand, when using the sum array, we have only 2 writes at the end of the force calculations. We could insist on minimizing the number of used registers, and going with the second approach, but then we would have to concider allocating shared memory for intermediate results and storing the final values into the global forces array. However, since we are already taking up most and simetimes all of the available shared memory for the quadtree, we stuck with the usage of registers in situations like this.

After calculating the forces, the next part of the simulation step is updating the positions of the bodies. This is consisted of several computations and can be grouped into a single kernel code.

*// defining dimensions for rest of the calculation*

blockSize **=** **64;**

dimBlock **=** dim3**(**blockSize**);**

*// depends on N\_THREADS for arbitrary number of threads approach*

dimGrid **=** dim3**((**N\_THREADS **+** blockSize **-** **1)** **/** blockSize**);**

updateAccVelPos**<<<**dimGrid**,** dimBlock**>>>(**forces\_d**,** masses\_d**,** accelerations\_d**,** velocities\_d**,** positions\_d**,** DELTA\_T**);**

cudaDeviceSynchronize**();**

To calculate the optimal blockSize, we took into the condideration two things. Hardware limits of the used GPU, provided using the cudaDeviceProperties() function from the cuda\_runtime.h.

Device Name**:** NVIDIA T600

Total Global Memory**:** **3696** MB

Max Threads per Block**:** **1024**

Max Threads per SM**:** **1024**

Max Blocks per SM**:** **16**

Warp Size**:** **32**

Registers per SM**:** **65536**

Shared Memory per Block**:** **49152** bytes

Shared Memory per SM**:** **65536** bytes

Max Warps per SM**:** **32**

And the number of registers used in the kernel function, provided using the –-ptxas-options=-v flag when comiling the code.

ptxas info **:** Compiling entry function '\_Z15updateAccVelPosPdS\_S\_S\_S\_d' **for** 'sm\_52'

ptxas info **:** Function properties **for** \_Z15updateAccVelPosPdS\_S\_S\_S\_d

**0** bytes stack frame**,** **0** bytes spill stores**,** **0** bytes spill loads

ptxas info **:** Used **43** registers**,** used **0** barriers**,** **368** bytes cmem**[0],** **40** bytes cmem**[2]**

Even though the kernel function has only two local variables, the number of used registers is 43. The reason for this is that other for local variables, the registers are used for storing temporary results, compiler optimizations and implicit varialbes such as threadIdx and blockIdx.

\_\_global\_\_ **void** updateAccVelPos**(double\*** forces**,** **double\*** masses**,** **double\*** accelerations**,** **double\*** velocities**,** **double\*** positions**,** **double** DELTA\_T**)** **{**

**int** idx **=** blockIdx**.**x **\*** blockDim**.**x **+** threadIdx**.**x**;**

**if** **(**idx **>=** N\_BODIES**)**

**return;**

**for** **(int** body\_i **=** idx**;** body\_i **<** N\_BODIES**;** body\_i **+=** N\_THREADS**)** **{**

accelerations**[**body\_i **\*** **2** **+** **0]** **=** forces**[**body\_i **\*** **2** **+** **0]** **/** masses**[**body\_i**];**

accelerations**[**body\_i **\*** **2** **+** **1]** **=** forces**[**body\_i **\*** **2** **+** **1]** **/** masses**[**body\_i**];**

velocities**[**body\_i **\*** **2** **+** **0]** **+=** accelerations**[**body\_i **\*** **2** **+** **0]** **\*** DELTA\_T**;**

velocities**[**body\_i **\*** **2** **+** **1]** **+=** accelerations**[**body\_i **\*** **2** **+** **1]** **\*** DELTA\_T**;**

positions**[**body\_i **\*** **2** **+** **0]** **+=** velocities**[**body\_i **\*** **2** **+** **0]** **\*** DELTA\_T**;**

positions**[**body\_i **\*** **2** **+** **1]** **+=** velocities**[**body\_i **\*** **2** **+** **1]** **\*** DELTA\_T**;**

**}**

**}**

To update the positions, we first need to update the accelerations, as well as velocities. Following the formuals of physics, this part of the computation is simple and straightforward. All of these arrays are stored in global memory, and since each thread is accessing unique locations, storing them into shared memory would not be beneficial. Regarding the coalescense, as threads are processing bodies which are stored sequentially in the arrays, the access of the global memory is coalesced.

**for (int step = 0; step < N\_SIMULATIONS; ++step) {**

**...**

*// needed for next iterations's tree creation on cpu*

cudaMemcpy**(** positions**.**data**(),** positions\_d**,** N\_BODIES **\*** N\_DIM **\*** **sizeof(double),** cudaMemcpyDeviceToHost**);**

**}**

*// deallocation of GPU memory*

cudaFree**(**masses\_d**);**

cudaFree**(**positions\_d**);**

cudaFree**(**velocities\_d**);**

cudaFree**(**accelerations\_d**);**

cudaFree**(**forces\_d**);**

cudaFree**(**quadtree\_d**);**

After updating the bodies positions, it is necessary to transfer them to the host memory, so that the new quadtree can be created in the next iteration. After finishing all the steps of the simulation, GPU memory is deallocated.

vidi dal da koristis onaj alat za racunanje dimenzija, treba da imas razloge tipa cesto se menja, mozda za force computing, a za ovaj drugi, mogu ja da isprobam pa da koristim te fiksne vrednosti

za posle:  
  
vidi kad budes pokretao koji su blcoksizevi imaju smisla, pa izmeni u teksu.

Pomeni ovaj info sa --ptxas-options=-v u delu sa rezultatima, koliko registara, onajs stack frame itd